**Carbon Dioxide Capture in NaOH-Impregnated Activated Carbon**

Prapatsorn Borisut1, Chaiyot Tangsathitkulchai1, Atichat Wongkoblap1, Aroonsri Nuchitprasitchai1 and Krittamet Phothong 1,2

1 School of Chemical Engineering, Institute of Engineering, Suranaree University of Technology, Muang District, Nakhon Ratchasima 30000, Thailand
2 Process Department, TTCL Public Company Limited, Serm-Mit Tower, Asoke Rd., North Klongtoey, Wattana, Bangkok 10110, Thailand
email for correspondence: atichat@sut.ac.th

Carbon dioxide (CO2) adsorption at high pressures by alkali-impregnated activated carbons were studied in this presentation. Four types of activated carbon were prepared with two-step activation method and activation combined with oxidation method [1] and then impregnated in different concentration of alkali solution of 1, 4, 7 and 10%. The results of CO2 adsorption at 0 ̊C up to saturated pressure show that the maximum adsorption capacity was obtained from the activated carbon prepared by activation combined with oxidation method with 180 minutes of total activation time, two cycles for oxidation and 1% NaOH impregnation. The BET surface area of all activated carbons decreased with an increase in NaOH loading. Micropore volume of all activated carbons is maximum when impregnated with 1% NaOH. It is seemed that the impregnation with appropriate NaOH loading can develop some micropore on activated carbon surface and lead to an increase in micropore volume.

**References:**

1. P. Lawtae, and C. Tangsathitkulchai, A New Approach for Controlling Mesoporosity in Activated Carbon by the Consecutive Process of Air Oxidation, Thermal Destruction of Surface Functional Groups, and Carbon Activation (the OTA Method). Molecules, 26 (2021).

**Acknowledgements:**
The authors gratefully acknowledge the financial support from the National Research Council of Thailand (NRCT) via the Royal Golden Jubilee (RGJ) Ph.D. scholarship, batch number 21, grant number PHD/0214/2561.